//Copyright (C)2014-2025 Gowin Semiconductor Corporation.
//All rights reserved. 
//File Title: Physical Constraints file
//Tool Version: V1.9.11.01 Education (64-bit)
//Part Number: GW2AR-LV18QN88C8/I7
//Device: GW2AR-18
//Device Version: C
//Created Time: Mon 04 28 14:13:08 2025

IO_LOC "ws2812_dout" 79;
IO_PORT "ws2812_dout" IO_TYPE=LVCMOS18 PULL_MODE=UP DRIVE=8 BANK_VCCIO=1.8;
IO_LOC "leds[5]" 20;
IO_PORT "leds[5]" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "leds[4]" 19;
IO_PORT "leds[4]" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "leds[3]" 18;
IO_PORT "leds[3]" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "leds[2]" 17;
IO_PORT "leds[2]" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "leds[1]" 16;
IO_PORT "leds[1]" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "leds[0]" 15;
IO_PORT "leds[0]" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "sig" 73;
IO_PORT "sig" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "start" 88;
IO_PORT "start" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "clk" 4;
IO_PORT "clk" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
