node n0 {
    type host
    network-config {
	hostname host1
	!
	interface eth1
	 ip address 192.168.64.254/18
	!
	interface eth0
	 ip address 192.168.0.254/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
    }
    auto_default_routes enabled
    canvas c0
    iconcoords {216 168}
    labelcoords {216 204}
    interface-peer {eth0 n2}
    interface-peer {eth1 n3}
}

node n1 {
    type host
    network-config {
	hostname host2
	!
	interface eth2
	 ip address 192.168.64.253/18
	!
	interface eth1
	 ip address 192.168.192.254/18
	!
	interface eth0
	 ip address 192.168.128.254/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
    }
    canvas c0
    iconcoords {624 168}
    labelcoords {624 204}
    interface-peer {eth0 n4}
    interface-peer {eth1 n5}
    interface-peer {eth2 n3}
}

node n2 {
    type lanswitch
    network-config {
	hostname switch1
	!
    }
    canvas c0
    iconcoords {72 264}
    labelcoords {72 287}
    interface-peer {e0 n0}
    interface-peer {e1 n7}
    interface-peer {e2 n6}
}

node n3 {
    type lanswitch
    network-config {
	hostname switch2
	!
    }
    canvas c0
    iconcoords {360 264}
    labelcoords {360 287}
    interface-peer {e0 n0}
    interface-peer {e1 n9}
    interface-peer {e2 n8}
    interface-peer {e3 n1}
}

node n4 {
    type lanswitch
    network-config {
	hostname switch3
	!
    }
    canvas c0
    iconcoords {600 264}
    labelcoords {600 287}
    interface-peer {e0 n1}
    interface-peer {e1 n11}
    interface-peer {e2 n10}
}

node n5 {
    type lanswitch
    network-config {
	hostname switch4
	!
    }
    canvas c0
    iconcoords {792 312}
    labelcoords {792 335}
    interface-peer {e0 n1}
    interface-peer {e1 n13}
    interface-peer {e2 n12}
}

node n6 {
    type pc
    network-config {
	hostname pc1
	!
	interface eth0
	 ip address 192.168.0.1/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
	ip route 0.0.0.0/0 192.168.0.254
	!
    }
    auto_default_routes enabled
    canvas c0
    iconcoords {24 456}
    labelcoords {24 487}
    interface-peer {eth0 n2}
}

node n7 {
    type pc
    network-config {
	hostname pc2
	!
	interface eth0
	 ip address 192.168.0.2/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
	ip route 0.0.0.0/0 192.168.0.254
	!
    }
    auto_default_routes enabled
    canvas c0
    iconcoords {168 504}
    labelcoords {168 535}
    interface-peer {eth0 n2}
}

node n8 {
    type pc
    network-config {
	hostname pc3
	!
	interface eth0
	 ip address 192.168.64.1/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
	ip route 0.0.0.0/0 192.168.64.253
	ip route 0.0.0.0/0 192.168.64.254
	!
    }
    auto_default_routes enabled
    canvas c0
    iconcoords {264 408}
    labelcoords {264 439}
    interface-peer {eth0 n3}
}

node n9 {
    type pc
    network-config {
	hostname pc4
	!
	interface eth0
	 ip address 192.168.64.2/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
    }
    auto_default_routes enabled
    canvas c0
    iconcoords {408 504}
    labelcoords {408 535}
    interface-peer {eth0 n3}
}

node n10 {
    type pc
    network-config {
	hostname pc5
	!
	interface eth0
	 ip address 192.168.128.1/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
    }
    auto_default_routes enabled
    canvas c0
    iconcoords {504 408}
    labelcoords {504 439}
    interface-peer {eth0 n4}
}

node n11 {
    type pc
    network-config {
	hostname pc6
	!
	interface eth0
	 ip address 192.168.128.2/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
    }
    auto_default_routes enabled
    canvas c0
    iconcoords {648 504}
    labelcoords {648 535}
    interface-peer {eth0 n4}
}

node n12 {
    type pc
    network-config {
	hostname pc7
	!
	interface eth0
	 ip address 192.168.192.1/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
    }
    auto_default_routes enabled
    canvas c0
    iconcoords {744 408}
    labelcoords {744 439}
    interface-peer {eth0 n5}
}

node n13 {
    type pc
    network-config {
	hostname pc8
	!
	interface eth0
	 ip address 192.168.192.2/18
	!
	interface lo0
	 type lo
	 ip address 127.0.0.1/8
	 ipv6 address ::1/128
	!
    }
    auto_default_routes enabled
    canvas c0
    iconcoords {840 504}
    labelcoords {840 535}
    interface-peer {eth0 n5}
}

link l0 {
    nodes {n2 n0}
    bandwidth 0
}

link l1 {
    nodes {n3 n0}
    bandwidth 0
}

link l2 {
    nodes {n4 n1}
    bandwidth 0
}

link l3 {
    nodes {n5 n1}
    bandwidth 0
}

link l4 {
    nodes {n13 n5}
    bandwidth 0
}

link l5 {
    nodes {n12 n5}
    bandwidth 0
}

link l6 {
    nodes {n11 n4}
    bandwidth 0
}

link l7 {
    nodes {n10 n4}
    bandwidth 0
}

link l8 {
    nodes {n9 n3}
    bandwidth 0
}

link l9 {
    nodes {n8 n3}
    bandwidth 0
}

link l10 {
    nodes {n7 n2}
    bandwidth 0
}

link l11 {
    nodes {n6 n2}
    bandwidth 0
}

link l12 {
    nodes {n1 n3}
    bandwidth 0
}

canvas c0 {
    name {Canvas0}
}

option show {
    interface_names yes
    ip_addresses yes
    ipv6_addresses yes
    node_labels yes
    link_labels yes
    background_images no
    annotations yes
    hostsAutoAssign no
    grid yes
    iconSize normal
    zoom 1.0
}

